Daniel Steele

Lab #4

There are four (4) steps that TCP servers go through to communicate. What are those steps, including the associated function calls (e.g., dosomething() )?

The four basic steps creating the socket for a server are the following

* Creating a socket : socket()
* Binding a socket to a port : bind()
* Listening to the port : listen()
* Accepting a connection : accept()

Each of these system calls also have their associated parameters that them where to access and store information that either is being returned or is needed for the function. One thing in particular that I found interesting is that you can specify the number of clients that can be in line to connect in the listen() call (Stevens, Fenner, & Rudoff., 2004).

**References**

Stevens, W. R., Fenner, B., & Rudoff, A. M. (2004). Unix network programing (3rd ed.). Boston, MA:

Pearson Education.